{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":141,"n_cols":10,"rows_kept":141,"merged":[[0,0,0,9],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,1,6],[1,7,1,8],[1,9,2,9],[140,0,140,2]],"flags":["formulas_cached_only"]}
["电气自动化设备询价清单"]
["序号","设备名称","规格或型号","单位","数量","重量(t)",null,"价格 (万元)",null,"备注"]
[{"$nulls":5},"单","总","单","总"]
["一","电气系统"]
[1,"电源进线柜1AP1","GGD 2200×800×800  (H×W×D)","台",1]
[2,"变频控制柜1AP2","GGD 2200×800×800  (H×W×D)","台",1]
[3,"变频控制柜1AP3","GGD 2200×800×800  (H×W×D)","台",1]
[4,"变频控制柜1AP4","GGD 2200×800×800  (H×W×D)","台",1]
[5,"变频控制柜1AP5","GGD 2200×800×800  (H×W×D)","台",1]
[6,"变频控制柜1AP6","GGD 2200×800×800  (H×W×D)","台",1]
[7,"变频控制柜1AP7","GGD 2200×800×800  (H×W×D)","台",1]
[8,"低压控制柜1AP8","GGD 2200×800×800  (H×W×D)","台",1]
[9,"低压控制柜1AP9","GGD 2200×800×800  (H×W×D)","台",1]
[10,"低压控制柜1AP10","GGD 2200×800×800  (H×W×D)","台",1]
[11,"低压控制柜1AP11","GGD 2200×800×800  (H×W×D)","台",1]
[12,"低压控制柜1AP12","GGD 2200×800×800  (H×W×D)","台",1]
[13,"低压控制柜1AP13","GGD 2200×800×800  (H×W×D)","台",1]
[14,"低压控制柜1AP14","GGD 2200×800×800  (H×W×D)","台",1]
[15,"低压控制柜1AP15","GGD 2200×800×800  (H×W×D)","台",1]
[16,"低压电容柜","2200×800×800","台",2]
[17,"操作箱","适用于直启电机","台",47]
[18,"操作箱","适用于软启变频电机","台",25]
[19,"检修箱","600×500×250","台",2]
[20,"电源进线柜2AP1","GGD 2200×800×800  (H×W×D)","台",1]
[21,"变频控制柜2AP2","GGD 2200×800×800  (H×W×D)","台",1]
[22,"变频控制柜2AP3","GGD 2200×800×800  (H×W×D)","台",1]
[23,"低压控制柜2AP4","GGD 2200×800×800  (H×W×D)","台",1]
[24,"低压控制柜2AP5","GGD 2200×800×800  (H×W×D)","台",1]
[25,"变频控制柜2AP6","GGD 2200×800×800  (H×W×D)","台",1]
[26,"变频控制柜2AP7","GGD 2200×800×800  (H×W×D)","台",1]
[27,"低压控制柜2AP8","GGD 2200×800×800  (H×W×D)","台",1]
[28,"低压控制柜2AP9","GGD 2200×800×800  (H×W×D)","台",1]
[29,"低压电容柜","2200×800×800","台",2]
[30,"操作箱","适用于直启电机","台",25]
[31,"操作箱","适用于软启变频电机","台",20]
[32,"检修箱","600×500×250","台",2]
[33,"电源进线柜3AP1","GGD 2200×800×800  (H×W×D)","台",1]
[34,"低压控制柜3AP2","GGD 2200×800×800  (H×W×D)","台",1]
[35,"低压控制柜3AP3","GGD 2200×800×800  (H×W×D)","台",1]
[36,"低压控制柜3AP4","GGD 2200×800×800  (H×W×D)","台",1]
[37,"低压控制柜3AP5","GGD 2200×800×800  (H×W×D)","台",1]
[38,"低压控制柜3AP6","GGD 2200×800×800  (H×W×D)","台",1]
[39,"低压控制柜3AP7","GGD 2200×800×800  (H×W×D)","台",1]
[40,"变频控制柜3AP8","GGD 2200×800×800  (H×W×D)","台",1]
[41,"变频控制柜3AP9","GGD 2200×800×800  (H×W×D)","台",1]
[42,"变频控制柜3AP10","GGD 2200×800×800  (H×W×D)","台",1]
[43,"低压控制柜3AP11","GGD 2200×800×800  (H×W×D)","台",1]
[44,"低压控制柜3AP12","GGD 2200×800×800  (H×W×D)","台",1]
[45,"低压电容柜","2200×800×800","台",2]
[46,"操作箱","适用于直启电机","台",66]
[47,"操作箱","适用于软启变频电机","台",10]
[48,"检修箱","600×500×250","台",2]
["二","PLC自控"]
[1,"工控机","i5处理器，8G ，1THD ，键盘、鼠标","台",6]
[2,"显示器","液晶 24英寸","台",6]
[3,"计算机操作台","单人位","台",6]
[4,"UPS电源","3KVA 30分钟","台",6]
[5,"PLC控制柜1","2200×800×800","台",3]
[6,"PLC控制柜2","2200×800×800","台",2]
[7,"PLC控制柜3","2200×800×800","台",2]
[8,"操作系统","windows10操作系统","套",6]
[9,"上位机软件 (正版)","WinCC V7.4组态+运行版","套",1]
[10,"上位机软件 (正版)","WinCC V7.4运行版","套",5]
[11,"下位机软件 (正版)","TIA博图 V14","套",1]
[12,"上位机软件 (用户程序)","Based On WinCC V7.4","套",6]
[13,"下位机软件 (用户程序)","TIA博图 V14","套",3]
["三","仪表"]
[1,"灰仓高低料位","阻旋料位开关","台",2]
[2,"烘干后建筑弃土仓高低料位","阻旋料位开关","台",2]
[3,"窑尾温度","耐磨热电偶 分度号：K,测量范围：0~1100℃","支",2]
[4,"窑头温度","热电偶 分度号：K,测量范围：0~1100℃","支",2]
[5,"冷却机引风管道温度","热电偶 分度号：K,测量范围：0~1100℃","支",2]
[6,"回转窑托轮温度","端面热电阻PT100","支",40]
[7,"冷却机托轮温度","端面热电阻PT100","支",8]
[8,"窑尾压力","微差压力变送器-500~0Pa","台",2]
[9,"窑头压力","微差压力变送器-300~300Pa","台",2]
[10,"冷却机引风管道压力","压力变送器-5kPa~0Pa","台",1]
[11,"谷糠风压力","压力变送器,测量范围：0~15kPa","台",2]
[12,"助燃风压力","压力变送器,测量范围：0~30kPa","台",2]
[13,"谷糠风流量计","V锥型 法兰安装，刻度流量：  0~4500m3/h  介质：空气，配差压变送器","台",2]
[14,"助燃风流量计","V锥型 法兰安装，刻度流量：  0~58.5m3/min，介质：空气，配差压变送器","台",2]
[15,"谷糠仓高低料位","阻旋料位开关","台",6]
[16,"烟室高低料位","耐高温射频导纳料位开关","台",8]
[17,"磷石膏缓存仓高低料位","阻旋料位开关","台",10]
[18,"料仓称重传感器","含3个称重传感器7.5t，1个数显表","套",5]
[19,"粉磨系统高低料位","阻旋料位开关","台",18]
[20,"6.26引风机进口温度","热电阻 分度号：PT100,测量范围：0~450℃","支",1]
[21,"成品系统高低料位","阻旋料位开关","台",34]
[22,"氨水罐温度","热电阻 分度号：PT100,测量范围：0~450℃","支",1]
[23,"SCR出入口烟气温度","热电偶 分度号：K,测量范围：0~1100℃","支",2]
[24,"布袋除尘器入口温度","热电阻 分度号：PT100,测量范围：0~450℃","支",1]
[25,"氨水卸载泵出口压力","0MPa~0.4MPa,含隔离针形阀，压力引管等","套",1]
[26,"氨水输送泵出口压力","0MPa~1.6MPa,含隔离针形阀，压力引管等","套",2]
[27,"SCR入口压力","微差压力变送器-1000~1000Pa","台",1]
[28,"SCR出口压力","压力变送器-3kPa~0Pa","台",1]
[29,"清洗水泵出口压力","0MPa~1.0MPa,含隔离针形阀，压力引管等","套",1]
[30,"布袋除尘器入口压力","压力变送器-5kPa~0Pa","台",1]
[31,"布袋除尘器出口压力","压力变送器-6kPa~0Pa","台",1]
[32,"循环碱水泵出口压力","0MPa~0.6MPa,含隔离隔膜阀","套",4]
[33,"排污泵出口压力","0MPa~0.6MPa,含隔离针形阀，压力引管等","套",2]
[34,"碱液输送泵出口压力","0MPa~0.4MPa,含隔离针形阀，压力引管等","套",2]
[35,"卸碱泵出口压力","0MPa~0.4MPa,含隔离针形阀，压力引管等","套",1]
[36,"碱洗塔除雾器差压","微差压力变送器0~1000Pa，隔离隔膜阀","套",1]
[37,"scr氨水管流量","0~100L/h","套",1]
[38,"碱液管道流量","0~0.5m³/h","套",1]
[39,"氨水储罐液位计","磁翻板液位计，0~4.5m","套",1]
[40,"旋风除尘器高料位","阻旋料位开关","套",2]
[41,"工艺水箱液位计","磁翻板液位计，0~2.8m","套",1]
[42,"循环池液位0~3.0m","雷达液位计，0~3.0m","套",1]
[43,"碱液罐液位计0~4.5m","磁翻板液位计，0~4.5m","套",1]
[44,"布袋灰斗高料位","阻旋料位开关","套",4]
[45,"布袋灰斗低料位","阻旋料位开关","套",4]
[46,"碱洗塔排出管PH计","0~14","套",1]
[47,"烟囱出口在线检测","TK-1000型 (常规监测)","套",1]
["四","电缆","详细设计出具清单，按实际长度结算"]
[1,"动力电缆","YJV-0.6/1KV 4×2.5","米",16000]
[2,"动力电缆","YJV-0.6/1KV 4×4","米",4800]
[3,"动力电缆","YJV-0.6/1KV 4×6","米",1600]
[4,"动力电缆","YJV-0.6/1KV 4×10","米",200]
[5,"动力电缆","YJV-0.6/1KV 4×16","米",1600]
[6,"动力电缆","YJV-0.6/1KV 3×25+1×16","米",900]
[7,"动力电缆","YJV-0.6/1KV 3×35+1×16","米",900]
[8,"动力电缆","YJV-0.6/1KV 3×50+1×25","米",200]
[9,"动力电缆","YJV-0.6/1KV 3×70+1×35","米",300]
[10,"动力电缆","YJV-0.6/1KV 5×2.5","米",900]
[11,"动力电缆","YJV-0.6/1KV 5×4","米",500]
[12,"动力电缆","YJV-0.6/1KV 5×6","米",100]
[13,"动力电缆","YJV-0.6/1KV 5×10","米",100]
[14,"动力电缆","YJV-0.6/1KV 3×120+1×70","米",200]
[15,"动力电缆","YJV-0.6/1KV 3×150+1×70","米",200]
[16,"动力电缆","YJV-0.6/1KV 3×185+1×95","米",600]
[17,"控制电缆","KVVP-500V 2×1.5","米",11440]
[18,"控制电缆","KVVP-500V 3×1.5","米",4340]
[19,"控制电缆","KVVP-500V 6×1.5","米",17180]
[20,"控制电缆","KVV-500V 8×1.5","米",10140]
[21,"控制电缆","KVV-500V 10×1.5","米",10400]
["五","桥架辅材",null,"批",1]
["六","电气施工图设计"]
["七","运输+卸车","负责将货物运输至湖北省孝感市大悟县阳平镇 循环经济产业园，并将货物卸车至安装位置附 近，含卸车所用吊车、人工费用"]
["八","安装","含低压柜、PLC柜及仪表安装，低压进线柜以 下动力及控制电缆敷设及接线调试"]
["合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}